Files included in this package:

1. readme.txt  - this document
2. PowerIT-i05-7_0_2.firmware - firmware to upload to device.
3. mib_name_file - Management information block.  For use with an SNMP console.
4. csv_name_file - SNMP info in CSV format if the SNMP console does not accept the MIB.
5. oneview_mib_name - Aggregated device data MIB for use with an SNMP console.
6. oneview_csv_name - SNMP info (OIDs) in CSV format for aggregated device data.

WARNING:
  Please read through the instructions thoroughly before proceeding to update your unit.
  Failure to follow the instructions exactly MAY damage your unit and MAY VOID YOUR WARRANTY.

Instructions for updating your device:

To update the firmware on your device.

	Open a web browser and browse to your device.
    Log in as administrator.
	If currently running 5.x firmware, go to System > Utilities > Firmware Update, or if currently running 6.x firmware, go to Utilities > Firmware > Update.
	Under 'Firmware Update' click 'Select Upload File' and select the geist-i05-7_0_2.firmware file.
	Click 'Submit' and wait for a restart of the device.
	
Should you run into any trouble while updating, please contact us.
  Phone : 1 800 222 5877
  E-mail: Monitoring.Support@Vertiv.com
  Web   : www.vertiv.com/support

Download new firmware releases at www.vertiv.com

Version 7.0.2. Built on 08/12/2025
