VERTIV 
FIRMWARE RELEASE NOTES

AFFECTED MODELS: GXT5 5KVA-10KVA Lithium (MV)
GXT5LI-5000MVRT3UXLN
GXT5LI-6000MVRT3UXLN
GXT5LI-8000MVRT4UXLN
GXT5LI-10KMVRT4UXLN

NOTE:
Each release includes all the updates from previous releases.
Refer to the update procedure in the zip file for detailed update instructions.
---------------------------------------------------------------------------
2025-May RELEASE

FILES:
GXT5LI-MCUV200-DSPV170-5-10k MV.bin
GXT5LI-MCUV130.bin
GXT5_192VLI-EBC_MCUPV130.bin
GXT5_192VLI-EBC_MCUSV130.bin

1. Start with No Battery ENABLED by default.
2. Auto Restart without Battery ENABLED by default.
3. HID re-map.
4. Power Assist output voltage corrected.
5. Improved DSP Processor auto-reboot process. Unit will now log UPS state and transfer to bypass during DSP reboot.
6. Soften the transfer from (Internal) Bypass back to operation on inverter.

Note: To sync GXT5 LI MCU Firmware across all models, GXT5 LI MV Firmware has moved directly to V200.

---------------------------------------------------------------------------
2023-July RELEASE

FILES:
GXT5LI-MCUV160-DSPV160-5-10k MV.bin
GXT5LI-MCUV130.bin
GXT5_192VLI-EBC_MCUPV130.bin
GXT5_192VLI-EBC_MCUSV130.bin

1. Improved RDU101 web-interface active events log by removing "UPS Output on Inverter" alert.
2. Improved the Lithium battery parameters on the UPS LCD

Note: UPS DSPV150 was never released and released from V140 to V160

---------------------------------------------------------------------------
2022-August RELEASE

FILES:
GXT5LI-MCUV150-DSPV140-5-10k-MV.bin
GXT5_192VLI-EBC_MCUPV130.bin

1. Enabled the ability to update the BMS through the UPS communication cable to the EBCs.

---------------------------------------------------------------------------
2022-July RELEASE

FILES:
GXT5LI-MCUV130-DSPV130-5-10k-MV.bin
GXT5_192VLI-EBC_MCUPV120.bin

1. Initial Release.

---------------------------------------------------------------------------
